Final Report

Predicting Machine Failure Using Time Series Data

Contributors: Samuel Scovronski

Introduction

The data for this project was provided by Microsoft as part of their Azure Machine Learning sample experiments. It consists of hourly average telemetry data for 100 machines over 1 year, and their respective failure, maintenance, and error logs. This means there are 876,000 rows of telemetry data with a timestamp.

There are three groups that care about being able to predict failures or maintenance needs, but each group has the same common goals. The groups include manufacturing companies that use equipment in their production, companies that produce electronic or moving products, and consumers that use those electronic products. Their goals with these types of models are minimizing machine/product maintenance costs, minimizing unplanned downtime, and maximizing machine/product life. In other words, minimize the cost of ownership and the inconvenience of unplanned downtime

Problem Statement

Manufacturing companies want to be able to know when their manufacturing equipment will break down before it happens, while simultaneously minimizing the amount of time spent on maintenance of the equipment. When using the traditional preventative maintenance method for failure prevention, depending on the schedule, the company could be servicing the equipment too frequently or not frequently enough because it does not account for the natural variance between machines. If the machine is maintained too frequently the company will spend more time servicing the equipment, spend more on materials, and reduce the amount of time it could be used to produce more products. If not maintained enough, then some machines could experience a failure resulting in unplanned downtime and potentially causing a chain of failures in other parts resulting in more machine down time and more costly repairs.

Data Wrangling

The dataset provided by Microsoft contained 876,000 rows and 6 columns of telemetry data in a csv format. No information was provided about whether the data was generated or recorded from actual machines. Four of the columns consist of hourly average sensor data, while the other two columns mark the machine the data was recorded from, and a time stamp of when the data was recorded. There are also 4 additional csv files, that consist of maintenance logs, failure logs, error logs, and some basic metadata of each machine.

Upon initial inspection of the data, there were no major issues identified. There were no missing telemetry values or timestamps for every machine throughout the year. However, some of the column data types had to be converted. All timestamps had to be converted from a string to a DateTime, and the errorID values needed to have the non-numerical values stripped so the error number could be converted to an integer. With all issues resolved, the telemetry data needed to be transformed into rolling windows, since using a single instance of raw values is typically not strong enough to predict future failures.

Exploratory Data Analysis

During exploratory data analysis

Surprisingly, the computer age and model number seem to have no impact on the number of errors or failures that it experiences. In fact, there is no correlation between age and the number of failures, and on average a computer only experiences 0.12 more errors for every additional year old it is.

Figure : Number of Machine Failures vs. Machine Age





Figure : Count of each Error Type vs. Machine Age



Looking at the raw sensor data for individual machines there are noticeable spikes in the data, that become even more pronounced when the moving average is taken. Below are some graphs depicting the moving average of the telemetry data for a single machine, with varying window sizes. This begs the question, do these spikes occur before a failure, after a failure, or are failures not associated with these spikes. Overlaying the failure occurrences (orange dots) over the raw data we see that some of the failures occur near the time when the spikes occur, but it does not occur consistently.

Figure : Machine 99 Moving Average Telemetry Data






Figure : Raw Rotation Data for Machine 99 Overlaid with Failure Occurrences



Although it was not explicitly stated if the data was generated or measured on actual machines, it seems likely that the data was generated. The reason for the suspicion is that the data seems to be nearly perfectly normally distributed. The histogram below displays the distribution of all vibration values recorded for every machine.

Figure : Histogram of all Vibration Data



Modeling Setup & Results

Data Preprocessing

One of the first preprocessing steps typically required for time series data is ensuring that the timestep between samples is constant. This requires resampling of the data and then using an interpolation method, such as forward fill, linear interpolation, etc. If you do not want to have a constant timestep then you must divide your values by the timestep to get the instantaneous rate of change of your values.

The next typical preprocessing step for time series data is the windowing of the data, in which the past n rows of data are grouped together. The data is windowed because using instantaneous values is less helpful for predicting the future than using a couple of the most recent values. For this model, I used a constant step size between windows of 1, or in other words, the window was moved forward by one timestep for each window. Once the data is grouped into multiple windows, there is the option to either use statistical values or the raw values of each window as the features fed into the model.

Once the feature are created, then the data needs to be normalized and split into training and testing data. For this project the data was standardized, and then it was split 70/30 into training and test data, respectively.

Model Criteria and Baseline Model Results